|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ID No. | Location | Date | Hydrant Condition No Damage / Cracks | Hydrant head / Coupling / Cover (not Corroded) | Hose and Nozzle No damage | Hose correctly rolled | Valve operation working / water under pressure | Cabinet Door condition | Cabinet Box condition | ID is clear or not | Remarks / remedial action | Initials |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |

Notes: 1. Mark: () if Ok, (X) if Not Ok, (-) if Not Applicable 2) During inspection and testing, try to rectify the faults then and there. Cleaning also to be done 3) Any Answer Is (X) , then the same shall be brought to the attention of the Administration for immediate replacement / repair 4) Weekly summary of such faulty items shall be made available to the Administration and re-inspection and testing shall be done and recorded 5) Every Month end completed record shall be maintained in HSE. 6) Inspection shall be carried out by Supervisor In-charge / HSEO