|  |
| --- |
| Inspection Check List for Safety Signs And Barrier |
| Date & time of Inspection: Location of Inspection: |
| Inspected by (Name of Safety Personal): Name of Execution Person: |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Sr.**  **No.** | **Check points** | **Yes/**  **No** | **Corrective Action Required** | **Action By** | **Due Date** | **Status** |
| 1 | Is there a sign identifying the MSDS location? |  |  |  |  |  |
| 2 | Are evacuation routes posted and muster points identified? |  |  |  |  |  |
| 3 | Are emergency exits marked? |  |  |  |  |  |
| 4 | Are appropriate PPE signs posted in required areas (e.g., “Hearing Protection Required”, “Hard Hats Required”, “Safety Glasses Required”)? |  |  |  |  |  |
| 5 | Are chemicals appropriately labelled and marked (e.g., hazardous goods information)? |  |  |  |  |  |
| 6 | Are “No Smoking” signs posted in required areas? |  |  |  |  |  |
| 7 | Are “High Voltage” signs posted in required areas? |  |  |  |  |  |
| 8 | Are “H2S” signs posted in required areas? |  |  |  |  |  |
| 9 | Are “Speed Limit” signs posted in required areas? |  |  |  |  |  |
| 10 | Are road safety signs posted at appropriate locations? |  |  |  |  |  |
| 11 | Are “Confined Space” signs posted in required areas? |  |  |  |  |  |
| 12 | Are “First Aid” signs posted to identify the location of medical supplies? |  |  |  |  |  |
| 13 | Are warning/hazard signs posted in required areas (e.g., sharp turn, narrow road, overhead power lines, etc.)? |  |  |  |  |  |
| 14 | Are trucks carrying hazardous chemicals appropriately marked with hazardous goods information? |  |  |  |  |  |
| 15 | Are signs indicating direction to/ location of safety showers / eye washes in prominent / strategic locations? |  |  |  |  |  |
| 16 | Has a proper colour coding system or sign posting been practiced for pipelines and structures? |  |  |  |  |  |
| 17 | Are maximum height clearance signs posted at overhead pipeline racks, overhead electrical power lines, overpasses etc.? |  |  |  |  |  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | **BARRIERS** |  |  |  |  |  |
| 18 | Are barriers in place where required?   1. General Warning - red/white 2. Overhead Work - black/yellow 3. Commissioning - blue/white   Notation example: a / yes - b / no |  |  |  |  |  |
| 19 | Are barriers / warnings being observed?  Watch the area for several minutes to ascertain if barriers are being violated by “pass-thru” staff |  |  |  |  |  |
| 20 | Are barriers in a good state of repair?  Not falling down/adequate height, etc |  |  |  |  |  |
| 21 | Are barriers being erected BEFORE work starts – Crane work in particular! |  |  |  |  |  |
| 22 | If rebar is used to support temporary tape barriers is the rebar properly hooked or capped. |  |  |  |  |  |
| 23 | Are Excavations and Trenches provided with “solid” barriers per Project Requirement? |  |  |  |  |  |

Checked By ………………………………………………………………… Date………………………………

Signature:

HSE Officer Superintendent /Foreman