|  |
| --- |
| **Inspection Checklist for Electrical Equipment** |
| Date & time of Inspection: Location of Inspection: |
| Inspected by (Name of Safety Personal): Name of Execution Person: |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Sr.**  **No.** | **Check points** | **Yes/**  **No** | **Corrective Action Required** | **Action By** | **Due Date** | **Status** |
| 1 | Physical condition of Power Generator |  |  |  |  |  |
| 2 | Housekeeping near & Inside Power Generator |  |  |  |  |  |
| 3 | Outlets Condition |  |  |  |  |  |
| 4 | ELCB/RCD |  |  |  |  |  |
| 5 | Isolation Points |  |  |  |  |  |
| 6 | Panels Locked |  |  |  |  |  |
| 7 | Cable Connections |  |  |  |  |  |
| 8 | Cable Terminations |  |  |  |  |  |
| 9 | Cable Condition |  |  |  |  |  |
| 10 | Cable Capacity & Ratings |  |  |  |  |  |
| 11 | Cable Routings / Cable Management |  |  |  |  |  |
| 12 | Earthling for Distribution Boards |  |  |  |  |  |
| 13 | Earthling for Cabins/Offices |  |  |  |  |  |
| 14 | Earthling for Transformers / Generators |  |  |  |  |  |
| 15 | Electrical hand tool physical Condition |  |  |  |  |  |
| 16 | Electrical hand tool cable’s Double Insulated |  |  |  |  |  |
| 17 | Electrical hand tool Sockets and Fittings are healthy |  |  |  |  |  |

**Comments :**

Checked By …………………………………………………………… Date……………………………………….…………

Signature

HSE Supervisor Electrical CM / Engineer / Foreman